GPIO are already configure in the file board.c

if (port\_pin\_get\_input\_level(BUTTON\_0\_PIN) == BUTTON\_0\_ACTIVE) {

/\* Yes, so turn LED on. \*/

puts("button on ");

port\_pin\_set\_output\_level(LED\_0\_PIN, LED\_0\_ACTIVE);

} else {

/\* No, so turn LED off. \*/

puts("button off ");

port\_pin\_set\_output\_level(LED\_0\_PIN, !LED\_0\_ACTIVE);

}